# Blind Single-sideband Demodulation
MATLAB package for compensation for the artifacts introduced by single-sideband demodulation with a mismatched demodulating carrier frequency.  Developed by Mark Harvilla, but essentially a re-implementation of an earlier algorithm by R. J. Dick at RADC.

## Usage
  1. Create a control file within which each line has a format like:

		 `path/to/SSB-modulated/input1.wav,path/to/demodulated/output1.wav`

	2. Run `pmces(ctl,maxShift,fs)` where
	    * `ctl` is the control file created in step 1
			* `maxShift` is the estimated maximum frequency shift from baseband in Hz
			  (a good number is 200 for RATS channel-D data)
			* `fs` is the sampling frequency of all audio files
