The Panospheric Alternative

Convex mirror

Wide-angle converter

Transparent cylinder

Camera body

raw warped image unwarped image

Innovative optic captures 360^o azimuth, +90^o to -60^o elevation in single image

Dewarping provides panorama, avoids issue of parallax in camera ring

2k x 2k CCD yields good resolution at horizon and terrific resolution nearby

Electronic pan/tilt and zoom available in software