16x62 Robot Quick Reference

Basic Commands Methods of RobotController (for talking to the Robot)

int serialOpen()
int serialClose()
int turnSonarsOn()
int turnSonarsOff()
int GS()
int setVel(int leftVel, int rightVel)
int killMotors()
int setAccel(int leftAccel, int rightAccel)
int configureSonars(int firingRate, int[] sonarOrder)  -- 16 elements!!!
int setTimeout(int timeout)

Sensor Information: State_Array in RobotController

Index 1-16: The sixteen sonar values, starting out front, going counter-clockwise Index 17: X integrated position Index 18: Y integrated position Index 19: Theta integrated position Index 20: Right wheel measured velocity Index 21: Left wheel measured velocity Index 22: Bumper status

Other Commands

SonarConsole - makes a sonar graphic display

DrawSonars(your_RobotController) - method that redraws the sonars.