Page 1 of 2

Demonstration Configuration

S1 S2 S3 S4 S5 H1 H2 H3

H4 H5 H6

Page 2 of 2

TCP over Flow-Controlled ATM S1 S2 S3 S4 S5 H1 H2 H3

H4 H5 H6 W/O ATM FC: Not fair? and under utilization? over L45 with per-VC queueing? W/ ATM FC: Fair? and high utilization? No TCP time-out? No cell loss?

M1=16K

M4=4K L45 M2=16K

M3=16K

10 TCP Sessions