   Current working directory:  C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd
>>> #define _WB_RUNNING
>>> path c:\ixa_sdk_3.5\src\applications\enp2611_static_fwd\;c:\ixa_sdk_3.5\src\applications\enp2611_static_fwd\dispatch_loop\;c:\ixa_sdk_3.5\src\applications\enp2611_static_fwd\scripts\;c:\ixa_sdk_3.5\me_tools\bin\;%PATH%
   Path search list for finding files (use "path" cmd to change this):
       1:  c:\ixa_sdk_3.5\src\applications\enp2611_static_fwd
       2:  c:\ixa_sdk_3.5\src\applications\enp2611_static_fwd\dispatch_loop
       3:  c:\ixa_sdk_3.5\src\applications\enp2611_static_fwd\scripts
       4:  c:\ixa_sdk_3.5\me_tools\bin
       5:  .
       6:  C:\WINNT\system32
       7:  C:\WINNT
       8:  C:\WINNT\System32\Wbem
       9:  c:\matlab6p5\bin\win32
      10:  c:\IXP1200\bin
      11:  C:\IXA_SDK_3.5\me_tools\bin
   
>>> foreign_model loader_dll.dll LoaderDLL
   1 foreign model is registered:
      LoaderDLL:  init str = "";  handle = 0;  call priority = 0
>>> foreign_model "C:\IXA_SDK_3.5\me_tools\bin\PhyDevice.dll" PhyDevice "" 1
   Loading foreign model dll.
   2 foreign models are registered:
      PhyDevice:  init str = "";  handle = 1;  call priority = 1
      LoaderDLL:  init str = "";  handle = 0;  call priority = 0
>>> foreign_model "C:\IXA_SDK_3.5\me_tools\bin\PacketSim.dll" PacketSim "" 0
   3 foreign models are registered:
      PhyDevice:  init str = "";  handle = 1;  call priority = 1
      LoaderDLL:  init str = "";  handle = 0;  call priority = 0
      PacketSim:  init str = "";  handle = 2;  call priority = 0
>>> inst sausalito
>>> init
   
*****************************************************
*** MAC version POS/UTOPIA IXP2400 Apr 24 2003 10:23:45
*****************************************************
>>> if (state_type(sr_chip_name) == 0) string sr_chip_name = "";
   
>>> if (state_type(sr_chip_name_dot) == 0) string sr_chip_name_dot = "";
   
>>> @C:\IXA_SDK_3.5\me_tools\bin\init_functions_IXP2400.ind
   Current working directory:  C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd
   
   
   
   
   2
   4
   4
>>> set_clocks("", 800, 0x00040044, 66, 0x00ee0000);
   1
tc0.PLT0_T_CLK:0> reset_one_chip("");
Chip is B0
   Tristate threshold check disabled on 156 tristate nodes
   146684 non-tristate states were specified and ignored in "set_float_threshold" command.
   PLXX_PLL_OUTOF_RESET_R1APBH<0> = 0    (0)   (signal)
   State, "PLXX_PLL_OUTOF_RESET_R1APBH" is forced.
   sh.shac_core.scratch.sh_cap_csr.cap_strap_options_rph<30:0> = 0000007F    (127)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_RST_L<0> = 1    (1)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_GNT_L<1:0> = 3    (3)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_CBE_L<7:0> = FF    (255)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_FRAME_L<0> = 1    (1)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_IRDY_L<0> = 1    (1)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_TRDY_L<0> = 1    (1)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_STOP_L<0> = 1    (1)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_DSEL_L<0> = 1    (1)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_PERR_L<0> = 1    (1)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_REQ64_L<0> = 1    (1)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_ACK64_L<0> = 1    (1)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_REQ_L<1:0> = 3    (3)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_INTA_L<0> = 1    (1)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_SERR_L<0> = 1    (1)   (signal)
   pci_cluster.pci_pad_arch.bfm_write_PCI_INTB_L<0> = 1    (1)   (signal)
WARNING:  Deposit action to the non-primary input state, PASH_NRESET_L, may be lost during simulation; use "/force" switch to avoid this.
   PASH_NRESET_L<0> = 1    (1)   (signal)
   PASH_NRESET_L<0> = 0    (0)   (signal)
   State, "PASH_NRESET_L" is forced.
   State, "PASH_NRESET_L" is no longer forced.
WARNING:  Deposit action to the non-primary input state, PASH_NRESET_L, may be lost during simulation; use "/force" switch to avoid this.
   PASH_NRESET_L<0> = 1    (1)   (signal)
   State, "PLXX_PLL_OUTOF_RESET_R1APBH" is no longer forced.
WARNING:  Deposit action to the non-primary input state, PLXX_PLL_OUTOF_RESET_R1APBH, may be lost during simulation; use "/force" switch to avoid this.
   PLXX_PLL_OUTOF_RESET_R1APBH<0> = 1    (1)   (signal)
   sh.shac_core.scratch.scr_csr_wr_data_wph<31:0> = 01200000    (18874368)   (signal)
   State, "sh.shac_core.scratch.scr_csr_wr_data_wph" is forced.
   sh.shac_core.scratch.sh_cap_csr.vMoD_gate__15953<2:0> = 1    (1)   (signal:unnamed_state)
   State, "sh.shac_core.scratch.sh_cap_csr.vMoD_gate__15953" is forced.
   State, "sh.shac_core.scratch.sh_cap_csr.vMoD_gate__15953" is no longer forced.
   State, "sh.shac_core.scratch.scr_csr_wr_data_wph" is no longer forced.
   sh.shac_core.scratch.scr_csr_wr_data_wph<31:0> = 00000000    (0)   (signal)
   State, "sh.shac_core.scratch.scr_csr_wr_data_wph" is forced.
   sh.shac_core.scratch.sh_cap_csr.vMoD_gate__15953<2:0> = 2    (2)   (signal:unnamed_state)
   State, "sh.shac_core.scratch.sh_cap_csr.vMoD_gate__15953" is forced.
   State, "sh.shac_core.scratch.sh_cap_csr.vMoD_gate__15953" is no longer forced.
   State, "sh.shac_core.scratch.scr_csr_wr_data_wph" is no longer forced.
model comes out of reset
WARNING:  Deposit action to the non-primary input state, dc.ddr_ctrl.ddr_ctrl.dx_core.dx_csr.dx_csra_register, may be lost during simulation; use "/force" switch to avoid this.
   dc.ddr_ctrl.ddr_ctrl.dx_core.dx_csr.dx_csra_register<31:0> = 01A04008    (27279368)   (flip-flop)
WARNING:  Deposit action to the non-primary input state, dc.ddr_mem.cas_delay_ctrl, may be lost during simulation; use "/force" switch to avoid this.
   dc.ddr_mem.cas_delay_ctrl<1:0> = 1    (1)   (signal)
WARNING:  Deposit action to the non-primary input state, dc.ddr_ctrl.ddr_ctrl.dx_core.dx_csr.dx_csr_errtst_reg, may be lost during simulation; use "/force" switch to avoid this.
   dc.ddr_ctrl.ddr_ctrl.dx_core.dx_csr.dx_csr_errtst_reg<8:0> = 100    (256)   (flip-flop)
tc0.PLT0_T_CLK:276> tc0.t0.thc.ti.csr_cc_enable_cu_rt = 1;
   tc0.t0.thc.ti.csr_cc_enable_cu_rt<0> = 1    (1)   (flip-flop)
tc0.PLT0_T_CLK:276> tc0.t0.thc.td.parity_enable_r = 0;
   tc0.t0.thc.td.parity_enable_r<0> = 0    (0)   (flip-flop)
tc0.PLT0_T_CLK:276> tc0.t1.thc.ti.csr_cc_enable_cu_rt = 1;
   tc0.t1.thc.ti.csr_cc_enable_cu_rt<0> = 1    (1)   (flip-flop)
tc0.PLT0_T_CLK:276> tc0.t1.thc.td.parity_enable_r = 0;
   tc0.t1.thc.td.parity_enable_r<0> = 0    (0)   (flip-flop)
tc0.PLT0_T_CLK:276> tc0.t2.thc.ti.csr_cc_enable_cu_rt = 1;
   tc0.t2.thc.ti.csr_cc_enable_cu_rt<0> = 1    (1)   (flip-flop)
tc0.PLT0_T_CLK:276> tc0.t2.thc.td.parity_enable_r = 0;
   tc0.t2.thc.td.parity_enable_r<0> = 0    (0)   (flip-flop)
tc0.PLT0_T_CLK:276> set_dram_size("", 1, 64);
WARNING:  Deposit action to the non-primary input state, dc.ddr_ctrl.ddr_ctrl.dx_core.dx_csr.dx_csra_register, may be lost during simulation; use "/force" switch to avoid this.
   dc.ddr_ctrl.ddr_ctrl.dx_core.dx_csr.dx_csra_register<31:0> = 01A04008    (27279368)   (flip-flop)
WARNING:  Deposit action to the non-primary input state, dc.ddr_mem.cas_delay_ctrl, may be lost during simulation; use "/force" switch to avoid this.
   dc.ddr_mem.cas_delay_ctrl<1:0> = 1    (1)   (signal)
WARNING:  Deposit action to the non-primary input state, dc.ddr_ctrl.ddr_ctrl.dx_core.dx_csr.dx_csr_errtst_reg, may be lost during simulation; use "/force" switch to avoid this.
   dc.ddr_ctrl.ddr_ctrl.dx_core.dx_csr.dx_csr_errtst_reg<8:0> = 100    (256)   (flip-flop)
   -I- Only 64 MB DRAM size is supported for IXP2400 at this point.
   -I- DRAM has been set to 1 channels of 64MB each
   1
tc0.PLT0_T_CLK:276> set_sram_channel_size("", 0, 1, 32);
WARNING:  Deposit action to the non-primary input state, pads.pa_qdr0.qdr_select_bit, may be lost during simulation; use "/force" switch to avoid this.
   pads.pa_qdr0.qdr_select_bit<0> = 0    (0)   (flip-flop)
WARNING:  Deposit action to the non-primary input state, pads.pa_qdr0.sram_size, may be lost during simulation; use "/force" switch to avoid this.
   pads.pa_qdr0.sram_size<2:0> = 6    (6)   (flip-flop)
WARNING:  Deposit action to the non-primary input state, pads.pa_qdr0.num_srams, may be lost during simulation; use "/force" switch to avoid this.
   pads.pa_qdr0.num_srams<0> = 0    (0)   (flip-flop)
   SRAM channel 0 has been set to a total memory of 64MB across 1 sram.
   1
tc0.PLT0_T_CLK:276> set_sram_channel_size("", 1, 1, 32);
WARNING:  Deposit action to the non-primary input state, pads.pa_qdr1.qdr_select_bit, may be lost during simulation; use "/force" switch to avoid this.
   pads.pa_qdr1.qdr_select_bit<0> = 0    (0)   (flip-flop)
WARNING:  Deposit action to the non-primary input state, pads.pa_qdr1.sram_size, may be lost during simulation; use "/force" switch to avoid this.
   pads.pa_qdr1.sram_size<2:0> = 6    (6)   (flip-flop)
WARNING:  Deposit action to the non-primary input state, pads.pa_qdr1.num_srams, may be lost during simulation; use "/force" switch to avoid this.
   pads.pa_qdr1.num_srams<0> = 0    (0)   (flip-flop)
   SRAM channel 1 has been set to a total memory of 64MB across 1 sram.
   1
tc0.PLT0_T_CLK:276> load_ixc (0) "C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\list\packet_rx.list"
   Loaded ucode file, "C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\list\packet_rx.list", into "tc0.t0.tu.ram_ustore"
tc0.PLT0_T_CLK:276> load_ixc (1) "C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\list\packet_echo.list"
   Loaded ucode file, "C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\list\packet_echo.list", into "tc0.t1.tu.ram_ustore"
tc0.PLT0_T_CLK:276> load_ixc (2) "C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\list\packet_tx.list"
   Loaded ucode file, "C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\list\packet_tx.list", into "tc0.t2.tu.ram_ustore"
tc0.PLT0_T_CLK:276> load_uof("C:\\IXA_SDK_3.5\\src\\applications\\enp2611_static_fwd\\enp2611_static_fwd.uof", "");
   Loaded uof file, "C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\enp2611_static_fwd.uof", into microengine control store.
   1
tc0.PLT0_T_CLK:276> enable_microengine("", 0);
   tc0.t0.thc.TX_CTX_0_ENABLE_RT<0> is a synonym state to tc0.t0.__18<0>:
   tc0.t0.__18<0> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t0.thc.TX_CTX_0_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t0.thc.TX_CTX_1_ENABLE_RT<0> is a synonym state to tc0.t0.__18<1>:
   tc0.t0.__18<1> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t0.thc.TX_CTX_1_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t0.thc.TX_CTX_2_ENABLE_RT<0> is a synonym state to tc0.t0.__18<2>:
   tc0.t0.__18<2> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t0.thc.TX_CTX_2_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t0.thc.TX_CTX_3_ENABLE_RT<0> is a synonym state to tc0.t0.__18<3>:
   tc0.t0.__18<3> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t0.thc.TX_CTX_3_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t0.thc.TX_CTX_4_ENABLE_RT<0> is a synonym state to tc0.t0.__18<4>:
   tc0.t0.__18<4> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t0.thc.TX_CTX_4_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t0.thc.TX_CTX_5_ENABLE_RT<0> is a synonym state to tc0.t0.__18<5>:
   tc0.t0.__18<5> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t0.thc.TX_CTX_5_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t0.thc.TX_CTX_6_ENABLE_RT<0> is a synonym state to tc0.t0.__18<6>:
   tc0.t0.__18<6> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t0.thc.TX_CTX_6_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t0.thc.TX_CTX_7_ENABLE_RT<0> is a synonym state to tc0.t0.__18<7>:
   tc0.t0.__18<7> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t0.thc.TX_CTX_7_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
tc0.PLT0_T_CLK:276> enable_microengine("", 1);
   tc0.t1.thc.TX_CTX_0_ENABLE_RT<0> is a synonym state to tc0.t1.__18<0>:
   tc0.t1.__18<0> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t1.thc.TX_CTX_0_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t1.thc.TX_CTX_1_ENABLE_RT<0> is a synonym state to tc0.t1.__18<1>:
   tc0.t1.__18<1> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t1.thc.TX_CTX_1_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t1.thc.TX_CTX_2_ENABLE_RT<0> is a synonym state to tc0.t1.__18<2>:
   tc0.t1.__18<2> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t1.thc.TX_CTX_2_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t1.thc.TX_CTX_3_ENABLE_RT<0> is a synonym state to tc0.t1.__18<3>:
   tc0.t1.__18<3> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t1.thc.TX_CTX_3_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t1.thc.TX_CTX_4_ENABLE_RT<0> is a synonym state to tc0.t1.__18<4>:
   tc0.t1.__18<4> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t1.thc.TX_CTX_4_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t1.thc.TX_CTX_5_ENABLE_RT<0> is a synonym state to tc0.t1.__18<5>:
   tc0.t1.__18<5> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t1.thc.TX_CTX_5_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t1.thc.TX_CTX_6_ENABLE_RT<0> is a synonym state to tc0.t1.__18<6>:
   tc0.t1.__18<6> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t1.thc.TX_CTX_6_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t1.thc.TX_CTX_7_ENABLE_RT<0> is a synonym state to tc0.t1.__18<7>:
   tc0.t1.__18<7> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t1.thc.TX_CTX_7_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
tc0.PLT0_T_CLK:276> enable_microengine("", 2);
   tc0.t2.thc.TX_CTX_0_ENABLE_RT<0> is a synonym state to tc0.t2.__18<0>:
   tc0.t2.__18<0> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t2.thc.TX_CTX_0_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t2.thc.TX_CTX_1_ENABLE_RT<0> is a synonym state to tc0.t2.__18<1>:
   tc0.t2.__18<1> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t2.thc.TX_CTX_1_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t2.thc.TX_CTX_2_ENABLE_RT<0> is a synonym state to tc0.t2.__18<2>:
   tc0.t2.__18<2> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t2.thc.TX_CTX_2_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t2.thc.TX_CTX_3_ENABLE_RT<0> is a synonym state to tc0.t2.__18<3>:
   tc0.t2.__18<3> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t2.thc.TX_CTX_3_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t2.thc.TX_CTX_4_ENABLE_RT<0> is a synonym state to tc0.t2.__18<4>:
   tc0.t2.__18<4> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t2.thc.TX_CTX_4_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t2.thc.TX_CTX_5_ENABLE_RT<0> is a synonym state to tc0.t2.__18<5>:
   tc0.t2.__18<5> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t2.thc.TX_CTX_5_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t2.thc.TX_CTX_6_ENABLE_RT<0> is a synonym state to tc0.t2.__18<6>:
   tc0.t2.__18<6> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t2.thc.TX_CTX_6_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
   tc0.t2.thc.TX_CTX_7_ENABLE_RT<0> is a synonym state to tc0.t2.__18<7>:
   tc0.t2.__18<7> = 1    (1)   (flip-flop)
   -----------------------------------------------------------
   tc0.t2.thc.TX_CTX_7_WAKEUP_EVENTS_RT<16:0> = 00001    (1)   (flip-flop)
tc0.PLT0_T_CLK:276> ref_data_set_enable(0);
   1
tc0.PLT0_T_CLK:276> enable_fifo_callback(0);
   1
tc0.PLT0_T_CLK:276> ps_set_random_seed(1088996651);
   0
tc0.PLT0_T_CLK:276> phy_define_device("x32MPHY4", 0, 4);
   0
tc0.PLT0_T_CLK:276> phy_set_device_rx_param(0, 1, 65536);
   0
tc0.PLT0_T_CLK:276> phy_set_device_rx_param(0, 2, 128);
   0
tc0.PLT0_T_CLK:276> phy_set_device_rx_param(0, 3, 1000);
   0
tc0.PLT0_T_CLK:276> phy_set_device_rx_param(0, 6, 96);
   0
tc0.PLT0_T_CLK:276> phy_set_device_rx_param(0, 7, 104);
   0
tc0.PLT0_T_CLK:276> ps_set_device_param(0, 1, 4);
   0
tc0.PLT0_T_CLK:276> ps_set_device_param(0, 3, 8);
   0
tc0.PLT0_T_CLK:276> phy_set_port_rx_protocol(0, 0, 2);
   0
tc0.PLT0_T_CLK:276> phy_set_port_rx_param(0, 1, 3, 900);
   0
tc0.PLT0_T_CLK:276> phy_set_port_rx_protocol(0, 1, 2);
   0
tc0.PLT0_T_CLK:276> phy_set_port_rx_protocol(0, 2, 2);
   0
tc0.PLT0_T_CLK:276> phy_set_port_rx_protocol(0, 3, 2);
   0
tc0.PLT0_T_CLK:276> phy_enable_device(0, 1);
   0
tc0.PLT0_T_CLK:276> phy_create_device(0);
   0
tc0.PLT0_T_CLK:276> ps_set_port_input_data_stream("C:\\IXA_SDK_3.5\\src\\applications\\enp2611_static_fwd\\streams\\e_ip_64_port_0.strm", 0, 0);
   0
tc0.PLT0_T_CLK:276> ps_set_port_data_stream_options(0, 0, 0, 1);
   0
tc0.PLT0_T_CLK:276> ps_set_port_input_logging("C:\\IXA_SDK_3.5\\src\\applications\\enp2611_static_fwd\\Device0_Port0_Rx.log", 0, 0);
   0
tc0.PLT0_T_CLK:276> ps_set_port_input_data_stream("C:\\IXA_SDK_3.5\\src\\applications\\enp2611_static_fwd\\streams\\e_ip_64_port_1.strm", 0, 1);
   0
tc0.PLT0_T_CLK:276> ps_set_port_data_stream_options(0, 1, 0, 1);
   0
tc0.PLT0_T_CLK:276> ps_set_port_input_logging("C:\\IXA_SDK_3.5\\src\\applications\\enp2611_static_fwd\\Device0_Port1_Rx.log", 0, 1);
   0
tc0.PLT0_T_CLK:276> ps_set_port_input_data_stream("C:\\IXA_SDK_3.5\\src\\applications\\enp2611_static_fwd\\streams\\e_ip_64_port_2.strm", 0, 2);
   0
tc0.PLT0_T_CLK:276> ps_set_port_data_stream_options(0, 2, 0, 1);
   0
tc0.PLT0_T_CLK:276> ps_set_port_input_logging("C:\\IXA_SDK_3.5\\src\\applications\\enp2611_static_fwd\\Device0_Port2_Rx.log", 0, 2);
   0
tc0.PLT0_T_CLK:276> phy_connect_device("", 0, 1);
   0
tc0.PLT0_T_CLK:276> phy_define_device("x32MPHY4", 1, 4);
   0
tc0.PLT0_T_CLK:276> phy_set_device_tx_param(1, 1, 16384);
   0
tc0.PLT0_T_CLK:276> phy_set_device_tx_param(1, 2, 8192);
   0
tc0.PLT0_T_CLK:276> phy_set_device_tx_param(1, 3, 1000);
   0
tc0.PLT0_T_CLK:276> phy_set_device_tx_param(1, 6, 96);
   0
tc0.PLT0_T_CLK:276> phy_set_device_tx_param(1, 7, 104);
   0
tc0.PLT0_T_CLK:276> ps_set_device_param(1, 2, 4);
   0
tc0.PLT0_T_CLK:276> ps_set_device_param(1, 3, 8);
   0
tc0.PLT0_T_CLK:276> phy_set_port_tx_protocol(1, 0, 2);
   0
tc0.PLT0_T_CLK:276> phy_set_port_tx_protocol(1, 1, 2);
   0
tc0.PLT0_T_CLK:276> phy_set_port_tx_protocol(1, 2, 2);
   0
tc0.PLT0_T_CLK:276> phy_set_port_tx_protocol(1, 3, 2);
   0
tc0.PLT0_T_CLK:276> phy_create_device(1);
   0
tc0.PLT0_T_CLK:276> ps_set_port_output_logging("C:\\IXA_SDK_3.5\\src\\applications\\enp2611_static_fwd\\Device1_Port0_Tx.log", 1, 0);
   0
tc0.PLT0_T_CLK:276> ps_set_port_output_logging("C:\\IXA_SDK_3.5\\src\\applications\\enp2611_static_fwd\\Device1_Port1_Tx.log", 1, 1);
   0
tc0.PLT0_T_CLK:276> ps_set_port_output_logging("C:\\IXA_SDK_3.5\\src\\applications\\enp2611_static_fwd\\Device1_Port2_Tx.log", 1, 2);
   0
tc0.PLT0_T_CLK:276> ps_set_port_output_logging("C:\\IXA_SDK_3.5\\src\\applications\\enp2611_static_fwd\\Device1_Port3_Tx.log", 1, 3);
   0
tc0.PLT0_T_CLK:276> phy_connect_device("", 1, 2);
   0
tc0.PLT0_T_CLK:276> phy_set_sim_options(0, 1, 1);
   0
tc0.PLT0_T_CLK:276> ps_set_logging_options(1, 1);
   0
tc0.PLT0_T_CLK:276> ps_enable_logging(1);
   0
tc0.PLT0_T_CLK:276> @C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\Scripts\wb_settings.ind
   Current working directory:  C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd
tc0.PLT0_T_CLK:276> @C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h
   Current working directory:  C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd
WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 99 -- Text following #endif is ignored
#endif /* USE_IMPORT_VAR */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 108 -- Text following #endif is ignored
#endif /* USE_IMPORT_VAR */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 145 -- Text following #endif is ignored
#endif /* USE_IMPORT_VAR */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 157 -- Text following #endif is ignored
#endif /* USE_IMPORT_VAR */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 202 -- Text following #endif is ignored
#endif /* USE_IMPORT_VAR */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 221 -- Text following #endif is ignored
#endif /* USE_IMPORT_VAR */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 239 -- Text following #endif is ignored
#endif /* USE_IMPORT_VAR */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 277 -- Text following #endif is ignored
#endif /* USE_IMPORT_VAR */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 307 -- Text following #endif is ignored
#endif /* USE_IMPORT_VAR */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 434 -- Text following #endif is ignored
#endif		/* PACKET_TX_IN_0_IND */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 464 -- Text following #else is ignored
#else	/* Used for micro-c */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 469 -- Text following #endif is ignored
#endif	/* IXP_MICROCODE */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 631 -- Text following #endif is ignored
#endif		/* PPP_RECEIVE */

WARNING:  File: C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\dispatch_loop\dl_system.h -- Line: 705 -- Text following #endif is ignored
#endif /* __DL_SYSTEM__H__ */

tc0.PLT0_T_CLK:276> @C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\Scripts\ether_init.ind
   Current working directory:  C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd
tc0.PLT0_T_CLK:276> @C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd\Scripts\system_setup.ind
   Current working directory:  C:\IXA_SDK_3.5\src\applications\enp2611_static_fwd

******************************************************

     System setup begin ...                           

******************************************************
   
   20480 = 0x00005000
   1
   0

*********************************************************

     System setup complete.                              

*********************************************************
tc0.PLT0_T_CLK:276> ubreak __wb_1_76 (1) 76#
   __wb_1_76      Breakpoint (enabled: evaluated on clk: tc0.PLT0_T_CLK)
          Breakpoints:  (1:7-0) = 76# 
