1-1

1

Introduction

Overview

This manual tells how to install an iWarp system. It is intended for use by Intel Customer Service

Engineers. The contents of the manual are as follows:

Chapter 1: Provides an overview of this manual, describes the tools required for unpacking and

installing an iWarp system, and provides an installation procedure flowchart.

Chapter 2: Tells how to inspect and unpack the iWarp system.

Chapter 3: Tells how to install and connect system cabinets and how to cable the iWarp system.

Chapter 4: Describes how to power up an iWarp system and run the system diagnostic tests.

T ools Required

Y ou need the following tools to unpack and install the iWarp system:

Unpacking 9/16 44 open-ended wrench

tape cutter

Installing 3/16 44 Allen wrench

5/32 44 Allen wrench

5/16 44 open, box, or ratchet wrench

5/16 44 thin-wall nut driver

small straight-slot screwdriver

#1 small-tip Phillips screwdriver

#2 medium-tip Phillips screwdriver

Installation Procedur e

Figure 1-1 provides a flowchart of the installation procedure for the iWarp system. The detailed

instructions for each step of the procedure are provided in Chapters 2, 3, and 4.

NOTES

The iWarp system software must be installed before the system diagnostics

can be run. Use the iW arp System Software Installation Instructions to

install the software. (The instructions are packed in the carton with the

system software.)

An iWarp Sun Interface Board (SIB) must be installed in the Sun system

cardcage before you can connect the iW arp array to the Sun system. If the

SIB hasn’t been installed, you must do so before trying to perform the

procedures in Chapter 3 of this manual. The iW arp Sun Interface Board

Installation Manual tells how to install the SIB.

1-2

* PROCEDURES FOR THE

iW ARP SYSTEM

SOFTW ARE AND SUN

INTERF ACE BOARD (SIB)

The procedures for the iWarp System Cabinets

may be performed in parallel with the

procedures for the iWarp system software and

Sun Interface Board (SIB).

Y es File Claim

with Carrier

Unpack/Inspect

Shipment

Review

Site Layout

Plan

Move�Cabinets

to Installation

Area

Damage?

Multiple

Cabinets?

Y es Connect

Cabinets

No

Connect

Interface

Cabling

Connect

Inter–cabinet

Cabling

Apply Power

and Run

Diagnostics

Pass/Fail?

Fail Refer to

Chapter 4

Installation

Complete

No

* PROCEDURES FOR THE

iW arp SYSTEM CABINETS

Install iWarp

SW on the Sun

Install the SIB

in the Sun

* NOTE

Figur e 1-1: iWarp System Installation Procedur e