Object:

JACKET

CLARE

 Show Phases

  New Phase

   Redraw

 Instantiate

UnInstantiate

 Visual->LISP

LISP->Visual

  Data Flow

    Start

    Stop

Code Control:

Insert Delete Modify Move Copy

    Action Test Other Above Below

      JACKET1:XX  FLUSH JACKET1 ?

      JACKET:STEAM-HEAT

                            ?VENT := ?SELF!VENT
                            ?DRAIN := ?SELF!DRAIN
                            ?CONTROL-LOOP := ?SELF!CONTROL-LOOP
                            ?STEAM-SUPPLY := ?SELF!STEAM-SUPPLY

                             CLOSE-VALVE ?CONTROL-LOOP ? (UNDEFINED)

                            LISP: (DO-TO-ROUTE ?STEAM-SUPPLY OPEN)

                            LISP: (DO-TO-ROUTE ?DRAIN OPEN)
                            ?TEMP :=
                                         LISP: (NUMERICAL-QUERY Please specify target temperature:)
                            Setpoint ?CONTROL-LOOP to ?TEMP
                            Switch ?CONTROL-LOOP to AUTO
                            ?HOW-LONG :=
                                             LISP: (NUMERICAL-QUERY Please specify how long to heat (secs):)
                                     ?SELF!TEMP-MEASUREMENT!VALUE is equal to ?TEMP
                                     ?HOW-LONG

                            LISP: (DO-TO-ROUTE ?STEAM-SUPPLY CLOSE)

                            LISP: (DO-TO-ROUTE ?DRAIN CLOSE)
                            Switch ?CONTROL-LOOP to MANUAL

                             CLOSE-VALVE ?CONTROL-LOOP ? (UNDEFINED)

      JACKET:CIRCULATE-COOLING-WATER

                                         ?VENT :=

                                                      ?SELF!VENT
                                         ?COOL-WATER :=

                                                            ?SELF!COOL-WATER-SUPPLY
                                         ?COOL-WATER-RETURN :=

                                                                   ?SELF!COOL-WATER-RETURN

                                         LISP: (DO-TO-ROUTE ?VENT CLOSE)

                                         LISP: (DO-TO-ROUTE ?COOL-WATER OPEN)

                                         LISP: (DO-TO-ROUTE ?COOL-WATER-RETURN OPEN)

      JACKET:WAIT-TILL-EMPTY NOT-EMPTY is equal to EMPTY

      JACKET:FLUSH

                       CA :=
                                 LISP: (SELECTION-QUERY Select a flush method: (LIST COMPRESSED-AIR-SUPPLY GRAVITY) JACKET1)

                       VENT1 :=

                                             ?HOW is of type COMPRESSED-AIR-SUPPLY

                                             LISP: (SELECTION-QUERY Select a flushing route: (LIST VENT DRAIN) JACKET1)

                                             LISP: (SELECTION-QUERY Select a flushing route: (LIST DRAIN) JACKET1)
                       VENT1 := VENT1
                       DRAIN1 := DRAIN1
                       (LPS CWR CA CWS) := (LPS CWR CA CWS)
                                 CA is of type COMPRESSED-AIR-SUPPLY

                                          DRAIN1 :=

                                                                 VENT1 is of type DRAIN
                                                                 ?VENT
                                                                 DRAIN1

                                          LISP: (DO-TO-ROUTE VENT1 OPEN)

                                          LISP: (DO-TO-ROUTE CA OPEN)

                                          LISP: (DO-TO-ROUTE DRAIN1 CLOSE)

                                           WAIT-TILL-EMPTY JACKET1 ?

                                          LISP: (DO-TO-ROUTE ?VIA CLOSE)

                                          LISP: (DO-TO-ROUTE ?HOW CLOSE)

                                          ?OTHER :=

                                                                 ?VIA is of type DRAIN
                                                                 ?VENT
                                                                 ?DRAIN

                                          LISP: (DO-TO-ROUTE ?VIA OPEN)

                                          LISP: (DO-TO-ROUTE ?VENT OPEN)

                                          LISP: (DO-TO-ROUTE ?SERVICES CLOSE)

                                           WAIT-TILL-EMPTY JACKET1 ?

                                          LISP: (DO-TO-ROUTE ?VIA CLOSE)

                                          LISP: (DO-TO-ROUTE ?VENT CLOSE)